Home | Sitemap | Help
About Us | Products | Support | Contact Us
Baja 65
Don’t be fooled by the size of the Dune 65. This kart has the power and performance of some karts twice its size. A 6.5 HP four stroke engine with automatic clutch provides lightning fast throttle response. The unique mono shock suspension give a surprisingly smooth ride on flat to moderate terrain.
ENGINE
• | 6.5 HP Recoil Start
• | Four-Stroke
• | On/Off Button
• | Automatic Clutch Drive
SEATING
• | Single Bucket Seat
• | Three-Point Restraint Harness
CHASSIS
• | Length: 60”
• | Width: 36”
• | Height: 50”
• | Ground Clearance: 6”
• | Front Tire: 4.10 - 4
• | Rear Tire: 4.10 - 4
PERFORMANCE
• | PERFORMANCE
• | Suspension Type: Mono Shock
Dune 150
The Dune 150 is a machine built for serious off-road fun. Powered by a 150cc four cycle electric start engine with automatic CVT drive with reverse. Hydraulic 4-wheel braking and smooth and responsive long travel front and rear hydraulic suspension.
ENGINE
• | Engine Type – 150cc four-stroke
• | Starter – Electric Start
• | Ignition – Keyed
• | 1.75 Gallon Fuel Tank
DRIVETRAIN
• | Final Drive – Chain
• | Transmission – Fully Automatic CVT
SUSPENSION
• | Front Suspension – Dual A-Arm
• | Rear Suspension – Swing Arm
• | Suspension Travel (Front) – 8"
• | Suspension Travel (Rear) – 6"
BREAKING
• | Front Brakes – Dual Hydraulic Disc
• | Rear Brake – Oversized Hydraulic Disc
| Parking Brake – Lever Actuated
TIRES
• | Front – 19 x 8 – 7 Knobby
• | Rear– 22 x 11 – 10 Knobby
OTHER
• | Color – Red
• | Dual Bucket Seats with Headrests
| Restraining System, Dual 4-Point
CHASSIS
• | Length – 86"
• | Width – 54"
• | Height – 55"
• | Seat to Pedal – 36" – 42"
• | Ground Clearance (Front) – 6.5"
• | Ground Clearance (Rear) – 10"
• | Turning Radius – 24"
• | Top Speed – 36 MPH
• | Dual Front Headlights, Rear Brake Lights
*It is recommended that this vehicle be operated by persons age 16 or older with proper safety equipment.
SF 90
Shift gears like a real off-road racer in the new Baja Shifter 90. This intermediate go-kart features two forward speeds and one reverse gear. Shifting is easy thanks to an automatic clutching system. The time tested 90cc four stroke electric start engine provides plenty of power for the toughest terrain.
ENGINE
• | 90cc Electric Start
• | Four-Stroke
• | Keyed On/Off
• | 2 Forward Speeds
• | 1 Reverse Speed
• | Floor Mounted Gear Shift Knob
• | 1.18 Gallon Fuel Tank
DRIVETRAIN
• | Dual Bucket Seat
• | Dual-Point Restraint Harness
CHASSIS
• | Length: 60”
• | Width: 44”
• | Height: 49”
• | Seat to Pedal: 27” to 31”
• | Ground Clearance: 4.75”
• | Front Tire: 14.5/7.00 – 6
• | Rear Tire: 16/8.00 – 7
PERFORMANCE
• | Top Speed: 25 MPH Approx.
• | Suspension Type Front: A-Arm
• | Suspension Type Rear: Swing Arm
• | Suspension Travel Rear: 3.5”
• | Suspension Travel Front: 3.5”
Home | About Us | Products | Services | Support | Contact Us | Policies
All contents © copyright 2005-2006 ReconOffRoad.com. All rights reserved.