Home | Sitemap | Help
About Us | Products | Support | Contact Us
Scooter 50cc Specification:
Engine Single: Cylinder, 4 Stroke, 49.7cc
Cooling: Air Cooled
Carburation: Single Walbro Carburetor
Max Speed: 40 MPH
Fuel Capacity: 1.5 Gallons
Max Weight Capacity: 300lbs
Ignition: CDI(Electric Start), Kick Start
Transmission: Automatic Clutchless Centrifugal Belt Drive
Frame: Steel
Front Suspension: Twin Telescopic Fork
Rear Suspension: Mono Shock
Front Brake: Hydraulic Disc Brake
Rear Brake: Drum Brake
Front Rim: 3"x10" Alloy
Rear Rim: 3"x10" Alloy
Front Tire: 3.0"x10"
Rear Tire: 3.0"x10"
Crated: 67"x23"x43" 260lbs
Scooter 150 Specifications
Engine: Single Cylinder: 4 stroke 149.7cc
Width: 22"
HP: 8.84HP
Length 67.5"
Battery Amp: 7
Height: 41.5"
Cooling: AIR
Wheel Base: 51.5"
Cylinder: 1
Seat Height 31"
Cycle: 4
Ground Clearance: 6"
Start Method: CDI, KICK
Dry Weight: 190LBS
Transmission: AUTOMATIC
Gross Weight: 360LBS
Oil Type: 10W-40
Oil Cap: 1.2L
Front Brake: DISC
Gas Tank: Cap 0.9 GALLON(S)
Front Suspension: TWIN
Muffler: SINGLE
Rear Rim/Tire: 4"-12"
Rear Brake: DISC
Rear Suspension: MONO
Home | About Us | Products | Services | Support | Contact Us | Policies
All contents © copyright 2005-2006 ReconOffRoad.com. All rights reserved.